VRMP Template – By Section
Step 5- Outcomes
•Inspection Schedule

| The same worksheet will also be placed here with noted frequency of inspection
| listed by each.
| The areas identified by the UTRI model that are Very High (red) are inspected
| yearly with any developments or requirements for mitigation noted and acted upon.
| Areas identified as High (orange) are inspected every 1-2 years, Moderate (yellow)
| areas every 3-5 years, and Low (green) areas every 5-7 years. Note on the worksheet
| that all road segments, at a minimum, get a drive by windshield survey after a severe
| storm event. You will most likely find trees in need of removal or pruning during the
| scheduled inspections.